

**Thermal Energy**

**Solution Card No.6: Optimizing losses of condensate return in the boiler by pressurizing the daily tank**

|  |  |  |
| --- | --- | --- |
| **Solution Card No.6: Optimizing losses of condensate return in the boiler by pressurizing the daily tank** | | |
| **Inputs** | | |
| Hotel | \*\*\* | |
| Boiler Type | Fire Tube Boilers / Water Tube Boilers | |
| Fuel Type | Natural Gas / Diesel / LPG | |
| No. Of Units | 1 | |
| **Assumptions** | | |
| Operating Condition | \*\*\* TPH @ \*\*\* bar | |
| Exchange Rate | 16 EGP/USD | |
| Consumption Profile | \*\*\* hr/day | \*\*\* days/year |
| **Constraints** | | |
| Fuel Prices | \*\*\* EGP/MBTU (2020/2021) | |
| Water Prices | \*\*\* EGP/m3 (2020/2021) | |
| **Proposed Solution** |  | |
| Condensate Losses in Tank Flowrate | \*\*\* ton/hr | |
| Condensate Losses in Tank Percentage | \*\*\* % | |
| Annual Energy Saving | \*\*\* kWh (\*\*\* MBTU) | |
| **Economic Features** | | |
| Average CAPEX | EGP \*\*\* | |
| Annual Savings | EGP \*\*\* | |
| Payback Period | \*\*\* year | |
| Lifetime | 15 years | |
| Annual CO2 Reduction | \*\*\* tCO2e | |