**Air Quality and Emissions**

**(AE02)**



|  |  |
| --- | --- |
| **Fact Sheet AE02: Keep the ventilation systems of odor generating areas separate from the hotel' main ventilation system** | |
| **Overview** | |
| *Objective* | To separate ventilation systems in the closed areas |
| *Action* | Install separate ventilation system for odor generating areas |
| *Key Challenges* | High CAPEX |
| **Process** | |
| *Complexity* | Moderate – install separate ventilation systems |
| *Equipment & Material* | Heating/ cooling equipment, fans, filters and ducts |
| *Human Resources* | HVAC Technicians in house team or HVAC maintenance companies |
| **Considerations** | |
| *Regulatory Aspects* | None |
| *Economic* | Moderate CAPEX, Moderate OPEX, Low savings |
| *Advantages* | Avoid any undesired odors in the closed areas |
| *Disadvantages* | Installation of new ventilation system |
| **Impacts** | |
| *Environmental* | None |
| *Employment Opportunities* | Moderate – technical labors |